id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
7980	Adams, Henry Charles	The Sewerage of Sea Coast Towns			.txt	text/plain	38118	1128	60	High water is two hours and a quarter after the current; therefore the latest time for the period of discharge would be from two hours and a half to half an hour before high water, but, as during the first quarter of an hour the movement of the current, though slight, would be in the opposite direction, it would be advisable to curtail the time of discharge, and say that it should be limited to between two hours and a quarter and half an hour before high water. In some cases gun-metal bolts are used, as they resist the action of sea water better than steel, but they add considerably to the cost of the outfall sewer, and the principal advantage appears to be that they are possibly easier to remove than iron or steel ones would be if at any time it was required to take out any pipe which may have been accidentally broken.	cache/7980.txt	txt/7980.txt
