        item: #1 of 7
          id: 37389
      author: Race, Joseph
       title: Chlorination of Water
        date: None
       words: 42921
      flesch: 62
     summary: | coli_ | Parts +------+--------+ Index | per +------+-------+ Index | per | Agar | Agar |per 100|million. | Agar | Agar |per 100|Million. |1
    keywords: + =; = +; = =; acid; action; ammonia; bacteria |; bleach; c. |; c.cms; cent; chlorination; chlorine; chlorine gas; chlorine water; coli; concentration; contact; cost; cubic |; dosage; effect; germicidal; hours |; hypochlorite; increase; liquid; matter; method; nil |; organisms; ottawa; p.p.m; period; plant; process; results; sodium; solution; table; temperature; treatment; typhoid; use; water |; | +; | b.; | neg; | pos; | |
       cache: 37389.txt
  plain text: 37389.txt

        item: #2 of 7
          id: 38455
      author: Conway, G. R. G. (George Robert Graham)
       title: ASCE 1193: The Water-Works and Sewerage of Monterrey, N. L., Mexico The 4th article from the June, 1911, Volume LXXII, Transactions of the American Society of Civil Engineers. Paper No. 1193, Feb. 1, 1911.
        date: None
       words: 45715
      flesch: 72
     summary: +-----+------------+---------+-----------+---------+----------+--------+ | | Monthly | Liters | Price for | Minimum | Rate for | Total | |Class| property | of | 1,000 | monthly | drainage | rate | | | rental. +----------+-----------+--------+-----------------------------+--------+ | | INTERNAL |Cost of | EARTHWORK AND LABOR: | Total | | | DIAMETER | mater- |-------+------------+--------| cost of| | | OF | ials | | Cost of |Cost of | sewer | | | SEWERS.
    keywords: + =; --------------+----------+-------+------------+--------+----------+ |; = +; = =; = centimeter; = inch; = |; boy |; caulkers |; city; cm =; concrete; cutter |; fig; foreman |; hour |; linear |; monterrey; plate; reservoir; rings |; river; sewer |; supply; total |; | +; | =; | cost; | diameter; | employees; | lead; | meter; | peons; | pesos; | pipe; | quantities; | rate; | south; | square; | water; | |
       cache: 38455.txt
  plain text: 38455.txt

        item: #3 of 7
          id: 45703
      author: Spon, Ernest
       title: Water Supply: the Present Practice of Sinking and Boring Wells With Geological Considerations and Examples of Wells Executed
        date: None
       words: 72891
      flesch: 66
     summary: +------+----------+ Cubic Feet | Laid | Laid in | of | Laid | Laid in | of | Dry. | | | | | | | | | | |Barnet, East | Herts.|Lion's Down | 122 | 270 | 162 | 230 | 130 | | | | |Shaft half steined, half iron cylinders.| | | | | | | | | | | Ditto, New | |Near Railway | 137 | 302 | 159 | 280 | 130 | | | |Station | | | | | | | | | | | | | | | |Battersea | S. |Jones's Works| 249 | -- | 249 | | | | | | | | | | | | | Ditto | |Beaufoy's | 240 | -- | 240 | -- | -- | | | |Works |Yield said to equal 15,000 gallons a | | | | | day.
    keywords: -----+-----+ |; boring; boundary |; clay |; fig; gallons |; grit |; hole; illustration; inches; lane |; london |; oolite |; park |; road |; series- |; slate |; strata; t. |; thames |; town |; union |; water; | +; | brickwork; | ditto; | e.; | feet; | ft; | k.; | m.; | marl; | minute; | mortar; | north; | pressure; | s.; | sandstone; | thickness; | |; | |beaumont; | |bottom; | |brewery; | |bromley; | |broxbourne; | |company; | |croydon; | |edgware; | |factory; | |good; | |gravesend; | |hall; | |hampstead; | |hill; | |house; | |mitcham; | |old; | |pinner; | |square; | |station; | |street; | |supply; | |through; | |woolwich; | |yield; |isleworth |; |near |; |reservoir |; |sand.|clay.| |; |tottenham |; |waterworks |; |workhouse |; |works |
       cache: 45703.txt
  plain text: 45703.txt

        item: #4 of 7
          id: 54454
      author: Boulnois, H. Percy (Henry Percy)
       title: Dirty Dustbins and Sloppy Streets A Practical Treatise on the Scavenging and Cleansing of Cities and Towns
        date: None
       words: 22585
      flesch: 53
     summary: This amounts to the | | | lecting house refuse | following:-- | |Name of Town.| and cleansing and +--------------+-------------+ | | watering streets and | Per 1,000 of | Per mile of | | | courts. | Description of | When paved.
    keywords: ashpit; authority; cart; chapter; cleansing; cost; day; ditto |; dust; house; public; refuse; sanitary; snow; streets; time; town; water; watering; work; | +; | |; |van |
       cache: 54454.txt
  plain text: 54454.txt

        item: #5 of 7
          id: 62605
      author: Simons, Joseph Winslow
       title: Sewage and Garbage Disposal on the Farm
        date: None
       words: 9378
      flesch: 68
     summary: Tile disposal fields, such as are used with septic tanks, and earth-pit privies accomplish this if the water table remains several feet below the surface and if the location is remote from water supplies. [Illustration] +---------------------------------------------------------------------------+ | CAPACITIES, DIMENSIONS, AND CONCRETE MATERIALS | | FOR SEPTIC TANKS SERVING INDIVIDUAL DWELLINGS | +---------+--------+--------------------------------+-----------------------+ |_Maximum
    keywords: disposal; feet; field; figure; joint; pipe; septic; sewage; sewer; soil; tank; tile; water; | +; | |
       cache: 62605.txt
  plain text: 62605.txt

        item: #6 of 7
          id: 62676
      author: Smith, Theobald
       title: Sewage Disposal on the Farm, and Protection of Drinking Water
        date: None
       words: 8260
      flesch: 73
     summary: Besides the protection of the ground-water near the well from pollution emanating from cesspools, etc., the surface of the ground about the well should be kept free from manure, slops, and other waste water; hence the well should not be dug under or close by the house,[3] nor should it be located in the barnyard, where the ground is usually saturated with manure. In the city the sanitary condition of homes is maintained chiefly by a system of cooperation and centralization which brings into existence extensive sewerage systems, water supplies, and the collection of house waste by public authority.
    keywords: closet; country; dry; earth; ground; house; sewage; soil; surface; water; wells
       cache: 62676.txt
  plain text: 62676.txt

        item: #7 of 7
          id: 7980
      author: Adams, Henry Charles
       title: The Sewerage of Sea Coast Towns
        date: None
       words: 38118
      flesch: 60
     summary: High water is two hours and a quarter after the current; therefore the latest time for the period of discharge would be from two hours and a half to half an hour before high water, but, as during the first quarter of an hour the movement of the current, though slight, would be in the opposite direction, it would be advisable to curtail the time of discharge, and say that it should be limited to between two hours and a quarter and half an hour before high water. In some cases gun-metal bolts are used, as they resist the action of sea water better than steel, but they add considerably to the cost of the outfall sewer, and the principal advantage appears to be that they are possibly easier to remove than iron or steel ones would be if at any time it was required to take out any pipe which may have been accidentally broken.
    keywords: cement; current; discharge; fig; float; flow; height; hour; moon; observations; outfall; point; position; sea outfall; sea water; sewage; sewers; storm water; surface; tide; time; velocity; water; water level; water mark; wind; | gallons; | nil; | |
       cache: 7980.txt
  plain text: 7980.txt

