id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajset-594	Xu, Zhi-Qiang; Gao, Yuan-Yuan	NEXT-GEN MAINTENANCE FOR URBAN RAIL TRANSIT: AN IOT-5G SYSTEM DESIGN	2023	11	.pdf	application/pdf	4619	215	47	D After each parameter is determined, the channel capacity G should be calculated as: 2 C 1+ ∑ηanEBan G AB D( , ) = ⋅lg( n an 2 ) (4) η C 1+ ∑∑ηanFFan a=1 n=1 This algorithm can determine the channel capacity of the power Internet of Things terminal task access, and can establish a secure communication channel. The impact of Internet of Things supported by emerging 5G in power systems: A review.	cache/ajset-594.pdf	txt/ajset-594.txt
