id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajset-1023	Opara, U V; Obiukwu , O O; Nwufo , O C; Ezeamaku , L U; Ezeaku , I I; Chiabuotu , C C; Ekpechi , D A; Okafor , B E	EFFECTS OF ANNEALING HEAT TREATMENT ON THE MECHANICAL AND MICROSTRUCTURAL CHARACTERISTICS OF MEDIUM CARBON STEEL.	2025	13	.pdf	application/pdf	5436	282	50	The muffle furnace was then set to the appropriate temperature range for medium carbon steel annealing, ranging between 600°C to 850°C. Abstract: The mechanical behavior and performance of medium carbon steel can be profoundly modified through thermal processing.	cache/ajset-1023.pdf	txt/ajset-1023.txt
