id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajset-567	Michael Brown, Alexander	THE FUTURE OF LOW SPEED SCRUBBING TECHNOLOGY	2023	14	.pdf	application/pdf	6950	328	57	With the assumptions of normal (Gauss) size distribution and spherical shape of the drops, it can be approximated as S~3.103/R~(400-800) m2/m3 depending on gas speed u~(10-20) m/s and volumetric flux of water ~(0.02-0.10) m3/m2s. In turn, both the overall cross-section of back-pipes Spipes~0.785d2( h)1/2/ (2g)1/2 (here = 1.8.( h)0.92 -0.61 is the coefficient of liquid discharge) and their total number m~ Spipes/0.785d2 are dictated by volumetric flux of water and gas speed u. The fixed centrifugal separator also has some special features, particularly the efficiency of phase separation, which is very sensitive with respect to the separator geometry, including number, height, and curvature of curvilinear blades.	cache/ajset-567.pdf	txt/ajset-567.txt
