




































    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

1 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

OPTIMIZING PRODUCTION COSTS: A REVIEW OF MODERN TOOLS 

AND TECHNIQUES IN MANUFACTURING 
 
1*Ezeaku I I, 2Onuoha G.O, 3Nwadinobi C.P and 4Opara V U 
1,3Department of Mechanical Engineering, Faculty of Engineering, Abia State University, Uturu, Nigeria. 
2,4Department of Mechanical Engineering, School of Engineering and Engineering Technology, Federal 

University of Technology, Owerri, Nigeria. 
*Corresponding author’s E-mail: ezeakuinnocentmnse@gmail.com. 

DOI: https://doi.org/10.5281/zenodo.15622483 

 

Abstract: Finding efficient ways to maximize production expenses has become even more vital given the rising 

complexity and competitiveness of world manufacturing. This study examines the most recent techniques and 

instruments employed to reduce costs without compromising operational efficiency or product quality. Although 

conventional techniques like lean manufacturing, Six Sigma, and just-in-time (JIT) approaches remain crucial, 

new developments in digital technology are altering the cost optimization method used. Real-time observation, 

predictive maintenance, and smart decision-making in production systems are made possible by new technologies 

including big data analytics, the Internet of Things (Iot), machine learning, and digital twins. Moreover, 

sophisticated cost models are increasingly generated and resource allocation is improved using computational 

intelligence techniques such as neural networks and genetic algorithms. This study provides a comprehensive 

review of both technology-based and conventional cost optimizing methods, evaluating their applicability for 

various sectors, effectiveness, and implementation difficulties. The review emphasizes significant trends and 

knowledge gaps by combining recent study with business practices, therefore offering a road map for future 

developments in cost-effective manufacturing. Particularly in the framework of Industry 4.0, the findings seek to 

help researchers, decision-makers, and practitioners select and apply suitable instruments for specific 

manufacturing environments and smart manufacturing systems. 

Keywords: Optimization, Production Costs, Cost-efficient manufacturing, decision-makers, Tools and 

Techniques 

 

Introduction 

In today's fiercely competitive industrial environment, manufacturers consider reducing production costs as a 

vital focus in order to achieve profitability, enhance operational efficiency, and boost market presence. The rising 

costs of raw materials, increased energy prices, higher labor costs, and the growing need for personalized products 

have put more pressure on manufacturers to create effective strategies for cost reduction (Gunasekaran et al., 

2001). Consequently, companies are utilizing a variety of contemporary tools and methods aimed at cutting waste, 

improving how resources are used, and streamlining processes while still ensuring product quality and satisfying 

mailto:topacademicjournals@gmail.com
mailto:ezeakuinnocentmnse@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

2 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

customers. 

Modern production cost reduction includes both conventional methods like lean manufacturing, Six Sigma, and 

just-in-time (JIT) systems, along with innovative technologies such as machine learning, big data analysis, digital 

twins, and the Internet of Things (IoT) (Womack & Jones, 2003; Lee et al. , 2015). These resources offer real-

time tracking and predictive insights that help manufacturers make knowledgeable choices and manage 

production resources effectively. In particular, techniques in Computational Intelligence (CI) have gained 

popularity for their potential to model intricate manufacturing systems and facilitate economical decision-making 

through smart automation (Jain et al., 2018). 

Even with a rising number of tools available, choosing the right and most effective techniques suitable for 

particular manufacturing settings is still difficult because of variations in production size, complexity, and levels 

of technology adoption. Hence, conducting a thorough examination of modern cost optimization methods and 

tools is crucial to grasp their functions, constraints, and implementation difficulties. This analysis intends to 

provide a detailed summary of present practices, shine a light on upcoming trends, and pinpoint areas lacking in 

current literature, thus offering helpful insights for both researchers and industry professionals aiming to enhance 

production costs in the age of smart manufacturing. 

Inventory Management  

In the present competitive business world, organizations need to manage inventories with efficient policies 

especially when the distribution network is dealing with deteriorating inventories ( Ahlaqqach et al.,2020). 

Sometimes due to high demand or season or the deteriorating nature of inventories, manufacturers increase their 

production and therefore need rented warehouse (RW) facility to manage a large number of inventories (Chang 

et al., 2020). Once the organization rents an extra facility to keep the extra number of inventories, the problem 

that they face is which inventories should be used first for minimum cost and minimum deterioration of 

inventories (Chang et al., 2020). The green supply chain is also a need as carbon factor is increasing in the 

environment and business firms are also responsible for carbon generation by manufacturing, transportation, 

warehousing, etc.; therefore, it needs to be controlled by effective policies. Government and policymakers initiate 

policies such as carbon tax, carbon cap, and trade and offset policies to control carbon factors (Ahlaqqach et al., 

2020). The deterioration process is a natural process that cannot be stopped but it can be minimized if deteriorating 

nature inventories are managed properly.  

Inspection is one such policy that is effective for deteriorating nature inventories. According to Bai et al., (2016), 

deteriorated inventories are removed from the supply chain at the initial stage, then it will not deteriorate other 

inventories by contact and the decaying process can be minimized to some extent. In the same way, separated 

deteriorated inventories can be utilized to earn revenue and also solve the problem of the disposal of decaying 

inventories. An inspection policy helps to reduce carbon emissions and helps to turn a supply chain into a green 

supply chain. Deterioration is a natural activity that must happen with decaying types of inventories (Pal et al., 

2015). It cannot be stopped but it can be minimized with some tools. Many researchers, policymakers, and 

organizations have given distinct policies, tools, and management areas that could be profitable for the firms to 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

3 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

handle such inventories. Many works have been conducted in this area with different policies. Pal et al., (2015), 

in their work defined a prepayment policy for retailers as a financial arrangement where customers are required 

to make a payment in advance before receiving goods or services. This policy is often used to manage credit risk, 

ensure cash flow, and reduce the risk of non-payment. Retailers might implement prepayment policies for various 

reasons, such as when dealing with new or untrusted customers, high-value products, or customized orders. It can 

also be used as a way to secure commitments from customers and manage inventory more effectively. 

Bai et al., (2016) is of the opinion that inspection policy for deteriorating inventories involves setting guidelines 

for the inspection, disposal, or handling of items that are prone to deterioration, spoilage, or obsolescence. This 

is particularly relevant for perishable goods, products with expiration dates, or items that lose value over time. 

Implementing an inspection policy can help reduce losses from holding inventory that is no longer usable or 

saleable due to deterioration. 

Muriana, (2016) stated that the actual behavior of the distribution network after applying an inspection policy can 

vary based on factors such as the nature of the products, the effectiveness of the policy implementation, the 

accuracy of demand forecasts, and the overall distribution structure. After applying an inspection policy for 

deteriorating inventories in a supply chain, several behaviors and outcomes may occur. The implementation of an 

inspection policy allows for more rigorous control over the quality and condition of inventory items. This helps 

to identify deteriorated items early enough and this prevents their inclusion in sales and reducing customer 

dissatisfaction (Bai et al., 2016). Also by identifying and disposing of deteriorating items promptly, the supply 

chain can minimize losses associated with holding inventory that can no longer be sold. The insights gained from 

the inspection policy can inform better demand forecasting and ordering decisions. This can lead to optimized 

inventory replenishment and reduced chances of overstocking items that might deteriorate (Panda and Modak, 

2017). Avoiding the sale of deteriorated items can enhance customer satisfaction and maintain the retailer's 

reputation for providing quality products. Also preventing the sale of deteriorated items can save costs related to 

customer complaints, returns, and refunds. Data collected through the inspection policy can be used to fine-tune 

inventory management strategies, including reorder points, safety stock levels, and replenishment schedules (Jing 

and Mu, 2019). According to Pand and Modak, (2017), implementing an inspection policy may require 

adjustments to processes and workflows to accommodate the identification, segregation, and disposal of 

deteriorating items. Khakzad and Gholamian, (2020) studied the prepayment policy for the retailer and the 

behaviour of distribution network after applying an inspection policy for deteriorating inventories. They were 

able to optimize the cost associated with the finished goods inventory. Halim et al., (2021) discussed a production 

opening inventory model for deteriorating items under overtime concept with price and available inventory 

focused demand. According to them, in the present combative and developing business world, it is a very 

challenging and tough task to manage decay type inventories without any loss. Moreover, a manufacturer may 

find it very costly to own a more spacious and well-established warehouse. In this situation, if the amount of 

manufactured inventories is more than the holding susceptibility of the owner warehouse (OW), the manufacturer 

will require a rented warehouse (RW) (Halim et al., 2021). Sometimes manufacturers feel the need for extra 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

4 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

production due to higher demand of inventories in the market and when manufacturer are dealing with 

deteriorating types of inventories, it necessary that production size be larger than demand of the market (Halim 

et al., 2021). Sometimes some seasonable products are manufactured before the season so as to fulfil market 

demand without delay. Some organizations manufacture inventories in RW and keep them in OW. Therefore, 

after placing them in RW, the next important policy is how to utilize these inventories, which means determining 

which inventories must be used first for maximum profit. Though it somewhat depends on factors such as the 

nature of the inventories and the rent of RW. Distinct supply chains adopt different policies but there are some 

policies that are established by policy makers and researchers. As well, these are also used by the market. 

Organizations are required to choose a dispatching policy that fits their supply chain and that can fulfil customer 

demand with minimum cost, less deterioration of inventory, and utilization of whole inventory without any loss 

(Maihami et al., 2019).  

For this, manufacturers should have enough knowledge about dispatching policies that suit their supply chain and 

provide maximum profit. Some of these policies are: 

(a) LIFO (last in first out) policy. This policy works with the concept that RW inventories should be used first 

as it reduces extra rent, which leads to minimum cost because it is an extra cost burden (Chakraborty et al., 2018). 

(b) FIFO (first in first out). This policy works with the concept that OW inventories should be used first as it 

reduces the deterioration rate, because the inventory that comes first is manufactured first so it will become 

deteriorated first, hence, when used first, it reduces the deterioration cost (Yu, 2019). There is one more concept 

behind this policy that some RWs provide better storage policies compared to OW which reduces deterioration. 

In RW, inventories can be kept fresh for a longer period and it minimizes deterioration cost and indirectly 

maximizes profit instead of greater cost of RW. In the FIFO policy, inventories that are kept first, must be utilized 

first. There are some RWs that charge less with a good quality of storage facilities that reduce deterioration so 

that it is more profitable for firms to use OW inventories. Many organizations work with this policy to make sure 

better originality of the stored inventory (Xu et al., 2017).  

(c) MFIFO (mix first in first out) policy. This works with the concept of the FIFO policy but with some 

modifications. In this policy, deteriorated inventories are replaced with RW so RW inventories are also 

simultaneously utilized. Xu et al., (2017) worked on this policy with a constant demand rate.  

(d) MLIFO (mix last in first out) dispatching policy. This policy works upon the LIFO policy with some 

modification. In this policy RW inventories are used first. Inventories from RW are sent to OW and then to the 

market. Some of the manufactures manufacture inventories in RW and then place them in owner warehouse. 

Notably, Xu et al., (2017) worked with this policy on deteriorating inventories. They also considered all the above 

policies and compared them using mathematical modeling in each case.  

(e) Mixed FIFO and LIFO policy. In this policy, both inventories are utilized simultaneously depending on the 

customer’s demand (Minner and Transchel, 2017). In this policy, OW inventories are utilized first but some 

fraction of inventories is replaced from RW. Thus, under this policy, both warehouses are used simultaneously 

and inventories are finished at the same time. Green supply chain means “integrate environmental thinking into 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

5 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

supply chain”. At the present time world business manufacturers, policymakers, and researchers are attracted to 

the problem of carbon emission during supply chain (Mishra et al., 2020). If the supply chain is dealing with 

deteriorating types of inventories then this problem requires more involvement. Policymakers and governments 

established a few policies to solve these problems such as carbon tax, cap and tax, offset policy and trade and cap 

etc. Huang. and Fang (2019) established a model considering the carbon emission regulation policy by using the 

game theory approach. Yu et al., 2020) studied and established a model with preservation technology for carbon 

emission considering demand as the function of stock and price. According to them, it was difficult to manage 

these inventories at a low cost but if these inventories deal with some special policies, then it is profitable. 

Inspection during supply chain to remove deteriorating inventories is one such tool that helps. Inspection policy 

is a kind of tool that converts a normal supply chain into a green supply chain. If during each cycle the inspection 

process is adopted, then these inventories can be separated at the initial stage (Mishra et al., 2020). This will help 

firms in two ways; one is that deteriorating inventories will not deteriorate other fresh inventories and the rate of 

decay can be minimized. The second is, if these deteriorating inventories are separated initially then it can be 

utilized for any purpose which helps to generate revenue. Inspection policy also helps in reducing emission (Yu 

et al., 2020). The separated products can be used for any other purpose based on the product or it can be sold as 

a product in the market at a low price so that it solves the disposal problem and reduces emissions. Thus, with 

this policy, the supply chain becomes a green supply chain. 

Simulation and Optimization Models 

Simulation optimization (SO) is simply refers as the optimization of an objective function subject to constraints, 

where both can be evaluated through stochastic simulation (Satyajith et al., 2016). Simulation optimization 

involves the search for those specific settings of the input parameters to a stochastic simulation such that a target 

objective, the function of the simulation output, is minimized. Simulation and optimization models are valuable 

tools used in cost optimization in manufacturing. These models enable manufacturers to analyze complex 

systems, simulate various scenarios, and identify optimal solutions for cost reduction and operational 

improvement. Simulation models replicate real-world processes using mathematical and statistical techniques 

(Satyajith et al., 2016). They simulate the behavior of a manufacturing system by capturing the interactions among 

various variables, such as resources, activities, and constraints. Simulation models can be used to assess the impact 

of different factors on costs, identify bottlenecks, and evaluate the effectiveness of potential cost optimization 

strategies. Key characteristics of simulation models are outlined by Andradottir (2006) as: 

1. Input Variables: Simulation models incorporate input variables such as production volumes, resource 

availability, demand patterns, and process parameters. 

II. System Representation: The model represents the manufacturing system's structure and processes, including 

production lines, workstations, material flows, and scheduling rules. 

III. Replication and Iteration: Simulation models are often run multiple times to generate statistical output and 

assess system performance under different scenarios. 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

6 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

IV. Analysis and Optimization: Simulation models enable the analysis of cost-related metrics, such as production 

costs, cycle times, inventory levels, and resource utilization. They can also be used to optimize system 

performance by identifying improvement opportunities and testing different cost-saving strategies. 

Optimization models form a significant area of research in various disciplines, including mathematics, operations 

research, engineering, and computer science. These models aim to find the best possible solution for a given 

problem by optimizing certain objective functions and subject to specific constraints (Deng and Ferris 2007). One 

widely studied category of optimization models is linear programming (LP), which involves linear relationships 

between variables and constraints. The simplex algorithm, proposed by George Dantzig in 1947, is a fundamental 

method used to solve LP problems (Dolan and More 2012). Nonlinear programming (NLP) extends optimization 

to handle non-linear objective functions and constraints. NLP models are commonly solved using techniques such 

as gradient-based methods, interior-point methods, or evolutionary algorithms. Integer programming (IP) deals 

with optimization problems where the decision variables must take integer values. These models are often more 

challenging to solve compared to linear programming. Additionally, there are specialized optimization models 

such as network optimization, stochastic optimization, dynamic programming, and convex optimization, each 

with their own specific techniques and applications. Optimization models use mathematical algorithms and 

techniques to determine the best allocation of resources and optimize decision-making (Dolan and More 2012). 

These models aim to find optimal solutions that minimize costs, maximize efficiency, or achieve other desired 

objectives. Optimization models can be used to address various cost optimization problems in manufacturing, 

including production planning, scheduling, capacity allocation, inventory management, and supply chain 

optimization. Optimization models define an objective function that quantifies the goal to be achieved, such as 

minimizing costs or maximizing profit. It also has decision variables which represent the decision options 

available, such as production quantities, resource allocations, or inventory levels. Optimization models 

incorporate constraints that reflect the limitations and requirements of the manufacturing system, such as capacity 

constraints, demand constraints, or resource availability constraints. Optimization models employ mathematical 

programming techniques, such as linear programming, integer programming, or dynamic programming, to find 

the optimal solution. 

It can be used to perform sensitivity analysis, which helps understand the impact of changes in input parameters 

on the optimal solution and cost outcomes (Wang and Pasupathy 2012). 

Simulation and optimization models offer several benefits for cost optimization in manufacturing. These models 

help identify cost-saving opportunities, optimize resource allocation, and streamline processes, leading to overall 

cost reduction. 

Optimization models optimize resource allocation, production planning, and scheduling to minimize costs and 

maximize operational efficiency. 

Simulation and optimization models can be integrated with other cost optimization techniques, such as activity-

based costing, lean manufacturing, or Six Sigma, to provide a comprehensive approach to cost optimization. For 

example, simulation models can evaluate the impact of lean initiatives or Six Sigma projects on costs and process 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

7 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

performance (Wang, 2012). Simulation and optimization models are powerful tools in cost optimization. They 

enable manufacturers to analyze complex systems, simulate scenarios, and identify optimal solutions for cost 

reduction, process improvement, and resource optimization. By leveraging these models, organizations can make 

data-driven decisions to enhance their cost competitiveness and operational efficiency. Fu et al., (2011) provides 

a comprehensive survey of the field and its scope in solving manufacturing cost problems. The paper listed 

different ways in which optimization and simulation interact and provides a very basic simulation output analysis 

and convergence theory for simulation optimization. Hong and Nelson (2009) classify simulation optimization 

problems into those with a finite number of solutions, continuous decision variables and discrete variables that 

are integer-ordered in cost problems. Birge and Louveaux (2011) maintained that simulation optimization, like 

stochastic programming attempts to optimize under uncertainty. However, stochastic programming differs in that 

it makes heavy use of the model structure itself. Derivative-free optimization (DFO) is sometimes referred to as 

black-box optimization method. Output variability is the key factor that distinguishes SO from DPO. As explained 

by Conn et al., (2009), some DPO algorithm under certain assumptions, expect rates that are closer to linear than 

quadratic and therefore early termination may be suitable. Policy gradient methods (Peters et al., 2013) are a 

subfield of reinforcement learning, where the set of all possible sequences of actions make up the policy space 

which is estimated and a gradient ascent-type method is then used to move to a local optimum. Discrete event 

simulations have been successfully used to model many real-world systems such as operations managements, 

queues and networks. The occurrence of events is modeled using probabilistic distributions in modelling the 

randomness (Peters et al., 2013). 

Cost Optimization tools and techniques in Manufacturing 

Cost optimization is a very important aspect of manufacturing operations (Chang. et al., 2020). The significance 

is presented in the following ways: It helps to improve profitability, competitive advantage, enhanced efficiency, 

sustainable operations, better decision making and adaptability of market changes (Zeng et al., 2020). Zeng et al., 

(2020) further explained thus: 

(i) Improved Profitability: Cost optimization directly impacts a company's profitability. By identifying and 

implementing measures to reduce production costs, companies can increase their profit margins and financial 

stability. This is especially crucial in industries with tight profit margins or intense competition. 

(ii) Competitive Advantage: In today's global marketplace, companies face intense competition. Implementing 

cost optimization strategies can provide a competitive edge by allowing companies to offer products at more 

competitive prices. This can help attract more customers and increase market share. 

(iii) Enhanced Efficiency: Cost optimization in manufacturing operations often involves streamlining processes, 

reducing waste, and improving efficiency. By identifying and eliminating inefficiencies, companies can improve 

production cycle times, reduce lead times, and enhance overall operational performance. 

(iv) Sustainable Operations: Cost optimization often involves reducing resource consumption, waste generation, 

and environmental impact. By implementing sustainable practices, companies can align their operations with 

environmental regulations and customer expectations, leading to improved brand reputation and customer loyalty. 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

8 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

(v) Better Decision-Making: Cost optimization requires a comprehensive understanding of production costs and 

factors influencing them. By analyzing cost data and implementing computational intelligence techniques, 

companies can gain insights that help in informed decision-making. This can involve identifying cost drivers, 

optimizing supply chain operations, or evaluating the cost-effectiveness of different manufacturing processes. 

(vi) Adaptability to Market Changes: Manufacturing companies must be agile and adaptable to changing market 

conditions, including fluctuating raw material costs, market demand shifts, or economic uncertainties. Cost 

optimization strategies enable companies to quickly respond to market changes by adjusting production processes, 

sourcing strategies, or pricing structures. Cost optimization in manufacturing operations is essential for improving 

profitability, competitiveness, operational efficiency, and sustainability. It allows companies to optimize their 

resources, enhance decision-making capabilities, and align their operations with market demands, leading to long-

term success in the manufacturing industry (Mohammadi et al., 2015). 

1. Activity-Based Costing (ABC) 

Activity-Based Costing (ABC) is a cost optimization technique that provides a more accurate and detailed 

understanding of costs by tracing them to specific activities within an organization. It is a valuable tool for 

identifying cost drivers, allocating resources effectively, and making informed decisions regarding product 

pricing, process improvements, and resource utilization (Ittner and Larcker 2011). 

Activity-Based Costing (ABC) emerged as a response to the limitations of traditional cost allocation methods, 

such as the volume-based allocation used in traditional costing systems. ABC recognizes that activities, rather 

than simple volume metrics, drive costs. It allocates costs based on the activities that consume resources and cause 

costs to be incurred. Ittner and Larcker (2011) argued that methodology of ABC involves the following steps: 

a. Identifying Activities: Activities are the fundamental actions or processes that occur within an organization, 

contributing to the creation of a product or service. 

b. Assigning Costs to Activities: Direct and indirect costs are assigned to each activity based on their consumption. 

c. Determining Cost Drivers: Cost drivers are the factors that influence the frequency or intensity of an activity. 

They provide a basis for allocating costs to cost objects (e.g., products, services, and customers) based on their 

utilization of activities. 

d. Allocating Costs to Cost Objects: Costs are allocated to cost objects using cost drivers and activity consumption 

data. 

Benefits of Activity-Based Costing: 

Enhanced Cost Accuracy: ABC provides a more accurate understanding of costs by attributing them to specific 

activities, enabling better cost control and cost reduction decisions (Ittner and Larcker 2011). ABC highlights the 

relationship between activities and costs, making it easier to identify areas of excessive costs or inefficiencies. 

Ittner and Larcker (2011) in their work, allocate resources more effectively and prioritize activities based on their 

impact on costs and performance of a manufacturing operations. They applied ABC facilitates in analysis of 

profitability at the product, customer, and market segment level, helping organizations focus on high-value 

products or customers which provides valuable cost information for decision-making, such as pricing decisions, 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

9 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

product mix optimization, process improvement initiatives, and outsourcing evaluations (Gunasekaran and Ngai 

2004). 

Implementing ABC requires significant effort in collecting accurate and reliable data on activity costs and their 

drivers. It can be challenging to obtain data from various sources and departments within the organization. 

Implementing ABC can be resource-intensive, requiring investments in technology, training, and data collection 

systems. The initial costs of implementing ABC may deter some organizations from adopting this approach (Ittner 

and Larcker 2011). Subjectivity in Cost Driver Selection: Choosing appropriate cost drivers involve subjective 

judgments and incorrect driver selection can lead to distorted cost allocations. Implementing ABC may face 

resistance from employees who are accustomed to traditional costing methods. Proper change in management and 

communication strategies is necessary to overcome this resistance (Gunasekaran and Ngai 2004). 

Integration with Other Techniques: 

ABC can be effectively integrated with other cost optimization techniques and tools to enhance decision-making 

and improve cost management. For example, ABC data can be integrated with simulation and optimization 

models to identify cost-efficient process configurations and resource allocations. Activity-Based Costing is a 

powerful cost optimization technique that provides organizations with a detailed understanding of costs and their 

drivers (Gunasekaran and Ngai 2004). By allocating costs based on activities, ABC enables informed decision-

making, better resource allocation, and improved profitability. However, implementing ABC requires careful 

planning, data collection, and consideration of organizational dynamics to overcome challenges and leverage its 

benefits effectively. 

Target Costing 

Target costing is a cost optimization technique that focuses on setting cost targets during the product design phase 

(Cooper and Slagmulder 2008). It is a proactive approach that aims to achieve desired profitability by considering 

customer requirements, competitor analysis, and market dynamics. Target costing involves a systematic process 

of cost planning, cost management, and value engineering throughout the product lifecycle. The primary objective 

of target costing is to determine the target cost for a product or service that will allow the organization to achieve 

its desired profitability while considering market conditions and customer expectations. Target costing provides 

understanding of customer needs, preferences, and price expectations through market research and customer 

feedback. Target costing enables setting a target price based on the market analysis, considering factors such as 

customer value perception, competition, and profitability goals (Gidiagba 2023). 

Benefits of Target Costing: 

According to Gidiagba (2023), the benefits of target costing include but not limited to the following:  

- Enhanced Cost Management: Target costing provides a systematic framework for managing costs 

throughout the product lifecycle, allowing organizations to proactively identify and control costs. 

- Customer Focus: By incorporating customer requirements and market dynamics into cost planning, target 

costing ensures that products are designed to meet customer needs and price expectations. 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

10 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

- Competitive Advantage: Target costing enables organizations to achieve cost leadership by optimizing 

costs while maintaining product quality and value. 

- Profitability Improvement: By aligning cost targets with profit objectives, target costing helps 

organizations improve profitability by achieving the desired profit margin. 

- Cross-Functional Collaboration: Target costing promotes collaboration between design, engineering, 

procurement, and manufacturing teams, leading to better cost control and innovation. 

Cost Optimization Techniques and Tools 

Simulation and Optimization Models 

Simulation and optimization models are valuable tools used in cost optimization in manufacturing. These models 

enable manufacturers to analyze complex systems, simulate various scenarios, and identify optimal solutions for 

cost reduction and operational improvement (Von- Ronne 2012). Simulation models replicate real-world 

processes using mathematical and statistical techniques. Simulation modelling and analysis is the process of 

creating and experimenting with a computerized mathematical model of a physical system (Chung 2010). They 

simulate the behavior of a manufacturing system by capturing the interactions among various variables, such as 

resources, activities, and constraints. Simulation models can be used to assess the impact of different factors on 

costs, identify bottlenecks, and evaluate the effectiveness of potential cost optimization strategies. Key 

characteristics of simulation models according to Van-Ronne (2012) include: 

1. Input Variables: Simulation models incorporate input variables such as production volumes, resource 

availability, demand patterns, and process parameters. 

II. System Representation: The model represents the manufacturing system's structure and processes, including 

production lines, workstations, material flows, and scheduling rules. 

III. Replication and Iteration: Simulation models are often run multiple times to generate statistical output and 

assess system performance under different scenarios. 

IV. Analysis and Optimization: Simulation models enable the analysis of cost-related metrics, such as production 

costs, cycle times, inventory levels, and resource utilization. They can also be used to optimize system 

performance by identifying improvement opportunities and testing different cost-saving strategies. Simulation 

models are categorized based on three dimensions, namely randomness, data organization and timing of change 

(Mourtzis et al., 2014). Simulation consists of an indispensable set of technological tools and methods for the 

successful implementation of digital manufacturing since it gives room for the experimentation and validation of 

process, configuration as well as system design. Simulation methods and tools are factory layout design, material 

and information flow design, manufacturing networks design, manufacturing systems planning and control, 

manufacturing networks planning and control, augmented and virtual reality in product and process design, 

planning and verification, ergonomics, robotics etc (Mourtzis et al., 2014). Out –bound manufacturing operations 

has a big challenge of identifying the benefits of collaboration. Confusion around the optimum number of partners, 

investment in collaboration and duration of partnership are some of the barriers of healthy collaborative 

arrangements that should be surpassed (Ramanathan 2014). Out-bound manufacturing operations is the value-

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

11 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

adding of activities from the initial raw materials to the ultimate consumption of the finished product spanning 

across multiple supplier- customer links (Dugal et al., 2011). 

Optimization models form a significant area of research in various disciplines, including mathematics, operations 

research, engineering, and computer science. These models aim to find the best possible solution for a given 

problem by optimizing certain objective functions and subject to specific constraints (Fazli-Khalaf et al., 2019). 

One widely studied category of optimization models is linear programming (LP), which involves linear 

relationships between variables and constraints. The simplex algorithm, proposed by George Dantzig in 1947, is 

a fundamental method used to solve LP problems. Nonlinear programming (NLP) extends optimization to handle 

non-linear objective functions and constraints. NLP models are commonly solved using techniques such as 

gradient-based methods, interior-point methods, or evolutionary algorithms. Integer programming (IP) deals with 

optimization problems where the decision variables must take integer values (Mourtzis and Nicholls 2020). These 

models are often more challenging to solve compared to linear programming. Additionally, there are specialized 

optimization models such as network optimization, stochastic optimization, dynamic programming, and convex 

optimization, each with their own specific techniques and applications. Optimization models use mathematical 

algorithms and techniques to determine the best allocation of resources and optimize decision-making (Mourtzis. 

and Nicholls 2020). These models aim to find optimal solutions that minimize costs, maximize efficiency, or 

achieve other desired objectives. Optimization models can be used to address various cost optimization problems 

in manufacturing, including production planning, scheduling, capacity allocation, inventory management, and 

supply chain optimization. Key characteristics of optimization models according to Mourtzis and Nicholls (2020) 

include:  

Objective Function: Optimization models define an objective function that quantifies the goal to be achieved, 

such as minimizing costs or maximizing profit.  

Decision Variables: These variables represent the decision options available, such as production quantities, 

resource allocations, or inventory levels.  

Constraints: Optimization models incorporate constraints that reflect the limitations and requirements of the 

manufacturing system, such as capacity constraints, demand constraints, or resource availability constraints.  

Solving Techniques: Optimization models employ mathematical programming techniques such as linear 

programming, mixed-integer programming and dynamic programming to find optimal solutions.  

Sensitivity Analysis: Optimization models can be used to perform sensitivity analysis, which helps understand 

the impact of changes in input parameters on the optimal solution and cost outcomes. Simulation and optimization 

models offer several benefits for cost optimization in manufacturing. These models help identify cost-saving 

opportunities, optimize resource allocation, and streamline processes, leading to overall cost reduction. 

Simulation and optimization models provide decision-makers with valuable insights and data-driven 

recommendations for making informed cost optimization decisions. Simulation models allow manufacturers to 

assess the impact of uncertainties, such as demand fluctuations or supply disruptions, on costs and performance. 

Simulation models assist in identifying process bottlenecks, inefficiencies, and improvement areas (Mourtzis and 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

12 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

Nicholls 2020). Optimization models optimize resource allocation, production planning, and scheduling to 

minimize costs and maximize operational efficiency. Simulation and optimization models can be integrated with 

other cost optimization techniques, such as activity-based costing, lean manufacturing, or Six Sigma, to provide 

a comprehensive approach to cost optimization. For example, simulation models can evaluate the impact of lean 

initiatives or Six Sigma projects on costs and process performance (Chang 2010). Simulation and optimization 

models are powerful tools in cost optimization. They enable manufacturers to analyze complex systems, simulate 

scenarios, and identify optimal solutions for cost reduction, process improvement, and resource optimization. By 

leveraging these models, organizations can make data-driven decisions to enhance their cost competitiveness and 

operational efficiency (Mourtzis and Nicholls 2020). 

Conclusion 

Manufacturers aiming to stay competitive have therefore an essential aim in lowering production costs. Great 

promise for cost reduction and efficiency improvement exists by mixing classic methods—such as lean 

manufacturing and Six Sigma—with modern technologies such as Io, machine learning, and big data analytics. 

Still, accomplishing this effectively calls for a tailored approach addressing issues particular to every sector. 

Future research should focus on improving these technologies and exploring their potential for collaborative use 

to maximize modern manufacturing systems for cost savings. Achieving continuous operational excellence in 

manufacturing will ultimately depend on a customized approach to cost control.  

References  

Ahlaqqach, M., Benhra, J., Mouatassim, S.and Lamrani, S. (2020). Closed loop location routing supply chain 

network design in the end of life pharmaceutical products. Supply Chain. Forum 21, 79–92.  

Andradottir S. (2006) recent nueral network simulation based optimization techniques: review of 

application.SIAM journal on optimization, 13(3), 666-701. 

Bai, Q., Xu, X., Xu, J., and Wang, D. (2016). Coordinating a supply chain for deteriorating items with multi-

factor-dependent demand over a finite planning horizon. Appl. Math. Model. 40, 9342–9361. [Cross-Ref]  

Birge J. and Louveaux F. (2011)) A robust dynamic programming approximation for a stochastic inventory 

routing problem. Transportation science, 34, 52-79. 

Chakraborty, D., Jana, D.K. and Roy, T.K. (2018). Two-warehouse partial backlogging inventory model with 

ramp type demand rate, three-parameter Weibull distribution deterioration under inflation and permissible 

delay in payments. Comput. Ind. Eng. 123, 157–179. [CrossRef]  

Chang, W. L., Huang, C. M. and Chen, J. H. (2020). Cost optimization of production planning for a cold chain 

system with carbon emission considerations. International Journal of Production Economics, 230, 107792. 

doi: 10.1016/j.ijpe.2020.107792 

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

13 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

Chung, C. (2010). Simulation modelling handbook. A practical approach, 1st Edition. CRC press Boca Rcton. 

20100. 

Conn A., Scheinberg K. and Vicente L. (2009) Sample path optimization in simulation. In: J. Tew. S. Manivannan, 

D. Sadowski, and Seila (Eds). Proceedings of 2008 winter simulation conference, pp.237-248. 

Cooper, G. and Slagmulder, E. (2008). Interorganizational cost management and relational context. Accounting, 

Organizations and Society, 28(1), 1-25. 

Deng G. and Ferris M., (2007). Multi-Objective linear programming model for a citrus supply chain network 

design: metaheuristic algorithms. J. Optim. Ind. Eng. 14, 137–154. 

Dolan M. and More J.,( 2012) Application of mixed integer linear programming in manufacturing cost reduction. 

. International Journal of Advanced science and technology. 28. 1-5. 

Dugal, I., Healy, M. and Tankentoo, S. (2011). Supply chain management: A challenge to change; Coopers and 

Lyband Report. 

Fazli-Khalaf, N., Khalilpourazari, S. and Mohammadi, M. (2019). Mixed robust possibilistic flexible chance 

constraint optimization model for emergency blood supply chain network design. Ann. Oper. Res. 283, 

1079–1109. 

. Fu M., Glover, F and April, J. (2011) Simulation optimization: A review, new developments and applications. 

In: M.E Kuhi,N.M. Steiger.,F.B Armstrong, and J. A Jones (Eds), proceedings of the 2011 winter 

simulation conference,pp.73-85. 

Gidiagba N. (2023) Application of target costing in manufacturing cost minimization in developing economy. 

International Journal of Engineering and Innovative Technology.(IJEIT). (4) 4, 2022-232. 

Gunasekaran, A., and Ngai, E. W. (2004). The successful management of a small logistics company through an 

activity-based costing approach. International Journal of Production Economics, 87(3), 321-331. 

Gunasekaran, A., Patel, C. and Tirtiroglu, E. (2001). Performance measures and metrics in a supply chain 

environment. Int. J. Oper. Prod. Manag. 21, 71–87. 

Halim, M.A., Paul, A., Mahmoud, M., Alshahrani, B., Alazzawi, A.Y. and Ismail, G.M. (2021). An overtime 

production inventory model for deteriorating items with nonlinear price and stock dependent demand. 

Alex. Eng. J. 60, 2779–2786. [Cross-Ref]  

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

14 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

Hong L. and Nelson B. (2009) A simulation-based procurement assessment framework in global wheat supply 

chain networks. J. Oper. Res. Soc. 74, 1242–1261.  

Huang, Y.S., Fang, C.C. and Lin, Y.A. (2019) Computers & Industrial Engineering Inventory management in 

supply chains with consideration of Logistics, green investment and different carbon emissions policies. 

Comput. Ind. Eng. 139, 106207. [Cross Ref]  

Ittner, C. D., and Larcker, D. F. (2011). Assessing empirical research in managerial accounting: A value-based 

management perspective. Journal of Accounting and Economics, 32(1-3), 349-410. 

Jain, S., Sekonyela, R., Knox, B., Palmer, J., Huttenlocher, A., Kabbage, M.and Keller, N. (2018) A Forward 

Genetic Screen in Zebrafish identifies the G-Protein-Coupled Receptor CaSR as a Modulator of 

Sensorimotor Decision Making Current biology: CB 28(9):1357-1369.E5 Journal. ID: ZDB-PUB-

180424-2. 

Jing, F. and Mu, Y. (2019). Forecast horizon for dynamic lot sizing model under product substitution and 

perishable inventories. Comput. Oper. Res. 110, 77–87. [Cross-Ref]  

Khakzad, A. and Gholamian, M.R. (2020). The effect of inspection on deterioration rate: An inventory model for 

deteriorating items with advanced payment. J. Clean. Prod. 254, 120117.  

Lee, G, Jui, Y and Veuio, M. (2015) Integrated Optimization models for the dynamic facility location and 

allocation problem. Int. J. Prod. Res. 46, 2070–2094. 

Maihami, R., Govindan, K. and Fattahi, M. (2019). The inventory and pricing decisions in a three-echelon supply 

chain of deteriorating items under probabilistic environment. Transp. Res. Part E Logist. Transp. Rev. 131, 

118–138. [Cross-Ref]  

Minner, S. and Transchel, S. (2017). Order variability in perishable product supply chains. Eur. J. Oper. Res. 260, 

93–107. [Cross-Ref]  

Mishra, U., Wu, J.Z. and Sarkar, (2020), B. Optimum sustainable inventory management with backorder and 

deterioration under controllable carbon emissions. J. Clean. Prod. 279, 123699. [Cross-Ref]  

Mohammadi, B., Taleizadeh, A.A., Noorossana, R. and Samimi, H. (2015). Optimizing integrated manufacturing 

and products inspection policy for deteriorating manufacturing system with imperfect inspection. J. 

Manuf. Syst. 37, 299–315.  

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

15 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

Mourtzis, D., Dowkas,M. and Bernidaki, D.(2014). Simulation in manufacturing: Review and challenges. The 

Elsevier B. V International scientific committee of the 8th International conference on digital Enterprise 

Technology- DET. DIO:10.1016/J.Procir.10.032 2212-8271. 

Mourtzis D. and Nicholls G.,( 2020).Optimal production-distribution planning in supply chain management using 

linear programming approach. In simulation conference procedings. 

Muriana, C. (2016). An EOQ model for perishable products with fixed shelf life under stochastic demand 

conditions. Eur. J. Oper. Res. 255, 388–396. [CrossRef]  

Pal, S., Mahapatra, G. and Samanta, G. (2015). A production inventory model for deteriorating item with ramp 

type demand allowing inflation and shortages under fuzziness. Econ. Model. 46, 334–345. 

Panda, S. and Modak, N. (2017). Coordination and benefit sharing in a three-echelon distribution channel with 

deteriorating product. Comput. Ind. Eng. 113, 630–645.  

Peters J., Vijayakumar S. and Schaal S., (2013) A locally derivative-free optimization (DFO) model for supplier 

selection in pharmaceutical industry. Applied mathematical modelling, 38, 3714-3726. 

Ramanathan, U. (2014). Performance of supply chain collaboration: A simulation study, Expert systems with 

Applications. (41) 1 210-220. 

Satyajith, A., Nikolaos, V., Bikram, S and Scott, J. (2016,). A generic simulation-based logistics assessment 

framework in global pharmaceutical supply chain networks. J. Oper. Res. Soc. 74, 1342–1360.  

Von Ronne, J.(2012). Simulation: Overview and Taxonomy, Presentation/ Technical report IEEE. 

Wang H. and Pasupathy R. (2012) A stochastic linear programming approach for supply chain network design 

under uncertainty. Eur. J. Oper. Res. 157, 93–112. 

Womeck, E. and Jones,N. (2003) A cost optimization technique of closed-loop supply chain considering customer 

satisfaction. International Journal of Production Economics, 226, 106685. doi: 

10.1016/j.ijpe.2020.107795. 

Xu, X. Bai, Q. and Chen, M. (2017). A comparison of different dispatching policies in two-warehouse inventory 

systems for deteriorating items over a finite time horizon. Appl. Math. Model. 41, 359–374. [Cross-Ref]  

Yu, C., Qu, Z., Archibald, T.W. and Luan, Z. (2020). An inventory model of a deteriorating product considering 

carbon emissions. Comput. Ind. Eng. 148, 106694. [Cross-Ref]  

mailto:topacademicjournals@gmail.com


    

 Academic Journal of Science, Engineering and Technology 

Vol. 10, Issue 2; May-June 2025; 

ISSN: 2837-2964 

Impact Factor: 7.67 

1252 Columbia Rd NW, Washington DC, United States 

https://topjournals.org/index.php/AJSET/index; mail: topacademicjournals@gmail.com 

 
 

 

 

16 | A c a d e m i c  J o u r n a l  o f  S c i e n c e ,  E n g i n e e r i n g  a n d  T e c h n o l o g y  

|  https://topjournals.org/index.php/AJSET 

Yu, J.C. (2019). Optimizing a two-warehouse system under shortage backordering, trade credit, and decreasing 

rental conditions. Int. J. Prod. Econ. 209, 147–155. [Cross-Ref] 

Zeng, S., Bai, X., and Wang, Y. (2020). A cost optimization model of closed-loop supply chain considering 

customer satisfaction. International Journal of Production Economics, 228, 107785. doi: 

10.1016/j.ijpe.2020.107785 

mailto:topacademicjournals@gmail.com

