id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajset-869	Debtera , Baru	COMPUTATIONAL FLUID DYNAMICS (CFD) SIMULATION OF A GAS-SOLID FLUIDIZED BED: RESIDENCE TIME VALIDATION STUDY 	2024	16	.pdf	application/pdf	6920	401	57	The fluidized bed is mainly selected for the mixture of solid catalyzed gas segment reactions because it can regulate the temperature of the reaction zone well, and the situations in fluidized bed reactors are approximately isothermal. Usually, fluidized bed reactors are chaotic in nature (Li et al., 2009).	cache/ajset-869.pdf	txt/ajset-869.txt
