id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajset-910	Okolotu , G.I.	FABRICATION OF BIOGAS DIGESTER AND PRODUCTION OF FUEL FROM ANIMAL DROPPINGS USING HIGH-DENSITY POLYETHYLENE AND POLYVINYL CHLORIDE 	2024	13	.pdf	application/pdf	5352	327	54	Four openings were provided: a substrate inlet (the coverable PVC pipe on the drum seal for pouring in solvents and solutions after corking the seal), substrate outlet (the PVC pump below the tank for removal of wastes), gas outlet (the PVC plastic pipe attached to the rubber tube, connected to the drum through the seal for the collection of produced gas from fermentation process for appropriate transmission of gas to the cylinder), and emergency pressure valve (the PVC pipe with tap connected, on the drum seal to regulate internal reaction within the gas production unit). i Heat Boiler: The heat boilers represent the simplest use of anaerobic produced gas.	cache/ajset-910.pdf	txt/ajset-910.txt
