




































American International Journal of Multidisciplinary Scientific Research 

Vol. 1, No. 1; 2018  

                                            Published by Centre for Research on Islamic Banking & Finance and Business, USA 

 

 

1 

 

Bandwidth Enhancement by Corner Truncation in Rectangular 

Patch Antenna 

 

M. Ramkumar Prabhu
1
, A.Rajalingam

2
 & J.Latha

2 

1
Apollo Engineering College, Chennai, India 

2
Shinas College of Technology, Sultanate of Oman 

Correspondence: M.Ramkumar, Apollo Engineering College, Chennai, India, Email: ramkumarprabhu.m@gmail.com 

 

 

Received:  July 6, 2018                                  Accepted: July 10, 2018                         Online Published: July 17, 2018                     

 

 

Abstract 

A method of improving operating bandwidth of a microstrip patch antenna by simply improving the structural shape, 

without affecting the size of an antenna is proposed in this paper. Simple calculations proved that Rectangular 

Microstrip Patch antenna of bandwidth 845.1 MHz can be efficiently transformed into microstrip patch antenna 

having bandwidth 9147.4 MHz . Two different approaches have been proposed and compared for better results. 

 

Keywords: Patch Antenna, Bandwidth improvement, RMSA(Rectangular Microstrip Patch Antenna) 

,UWB(Ultrawide Band) ,truncation. 

 

1. Introduction 

The recent progress in UWB wireless communications have remarkably increased the demand of wideband antenna 

with smaller dimensions than conventionally possible(H.N. Kritikos et al., 1990).The antenna size with respect to 

the wavelength is the parameter that will have influence on the radiation characteristics, gain and efficiency. 

Conventional microstrip antenna has limitation of narrow bandwidth, low gain and size of λ/2 (H.N. Kritikos et al., 

1990 - Werner, D. H et al., 2003). There are several techniques reported in the open literature to improve the 

bandwidth of the microstrip patch antenna such as insertion of air gap, stacking, ground coupling etc. The coupling 

effect is possible by changing the feed type and proper values of its parameters[Jiechen Ding, et al., 2007].CPW 

feed offers better resonant characteristics and impedance bandwidth (J. Liang et al., 2004 - J. Liang,et.al,2005). Use 

of metal flared array is very inefficient way to obtain wideband(Rick W. Kindt et al., 2010). Use of mathematically 

designed fractal structures is also a favorite method acquainted worldwide to obtain multiple bands and overlapping 

multiple bands will result in bandwidth improvement (Min Ding et. al. 2007). 

All methods of improving bandwidth mentioned above needs some kind of extra space by increasing size, or 

increase fabrication complexity as in case of fractals. Furthermore understanding of fractals involves complex 

mathematics. Keeping all above things in mind, this paper provides a simple but very efficient way to improve 

bandwidth. 3 types of antennas are considered; Type A is simple Rectangular Microstrip Patch Antenna with narrow 

bandwidth. Type B-Straight Edge Cut RSMA with slight improvement in bandwidth and Type C- Circular Edge Cut 

RSMA with more bandwidth improvement. All the results are obtained using AnSoft- HFSS v.11 

2. Simple RSMA Design 

2.1 Type A - Basic Rectangular Microstrip Patch Antenna) 

Basic Rectangular Microstrip Patch Antenna consists of simple Coplanar Microstrip Patch Antenna with no any 

modifications in patch or ground shape. Hereafter termed as simple RMSA. Design and dimensions are described in 

brief in next section. 

 

 



www.cribfb.com/journal/index.php/aijmsr           American International Journal of Multidisciplinary Scientific Research           Vol. 1, No. 1; 2018 

 

2 

 

2.2 Structure of simple RMSA 

 

                                                   

 

 

 

 

 

 

Figure 1. Structure of Basic Rectangular Microstrip Patch Antenna (Type A) 

CPW fed RMSA i.e. Rectangular Microstrip Patch Antenna is designed in HFSS on generally available FR4 
substrate of size 38mm X 43mm X 1.53mm and having dielectric constant of 4.4 and loss tangent (tan δ)=0.02. As 

shown in figure 1 both sides of actual radiating copper patch are chosen to be 18.4mm and structure is known to be 
coplanar as both ground and patch are on same plane. Thickness of the copper material is assumed 0.1mm which 
negligible in comparison with 1.53mm thickness of FR4 substrate material. As the structure is monopole, length of 
patch and ground are same. Dimensions of ground are 18.4mm X 16.9mm X 0.1mm. Feed width is 3.1mm fixed. 

Gap between feed and ground is optimized to 0.55mm and gap between patch and ground is 0.5mm. 

 

 

 

 

 

 

 

 

 

 

 

Figure 2. Return Loss vs. Frequency for simple RMSA (Type A) 

 

 

 

 

 

 

 

 

 

 

 

 

 

Figure 3.VSWR vs. Frequency for simple RMSA (Type A) 



www.cribfb.com/journal/index.php/aijmsr           American International Journal of Multidisciplinary Scientific Research           Vol. 1, No. 1; 2018 

 

3 

 

2.3 Simulation Results 

The structure is designed and simulated over HFSS v11. Figure 02 and 03 shows simulation results. The operating 

band of any antenna is described by return loss less than -10 dB or VSWR less than 2. Return loss of -10dB 

indicates that, 90% of the power fed to antenna is accepted and only 10% is reflected at the feed. Thus Return 

Loss<-10dB is universally accepted convention to decide operating band of an antenna. In figure 02 and 03, m1 is 

lower end operating frequency and m2 is higher end operating frequency, marking the -10dB crossing line. As can 

be seen from following figures, simple rectangular microstrip patch antenna covers bandwidth of 835.1 MHz, 

starting from 3.0526 GHz to 3.8877GHz. 

3. Bandwidth Increment by Cutting Corner Edges 

Bandwidth of operation of antenna is depend upon different parameters like size of an antenna, thickness and 

dielectric constant of substrate material used, proper impedance matching of connector and antenna etc. apart from 

these parameters, structure (M.Ramkumar Prabhu et al.,2017) of an radiating patch and ground also plays important 

role in deciding the bandwidth. Cutting corners of RMSA will induce more discontinuity in the flow of wave and 

increasing reflections will ultimately results in improved bandwidth. 

3.1 Type B-Straight Edge Cut Structure 

Keeping all parameters of design of simple RMSA constant, design is modified by cutting the corners of rectangular 

patch by straight edges. As shown in figure 04, antenna is of dimension (38.0mm X 43.0mm X 1.53mm) with patch 

(18.4mm X 18.4mm X 0.1mm) i.e. same as Type A. Corners of the radiating patch are truncated with variable length 

called ‘CUT’. This truncation is varied from 3.00mm to 7.00mm length with step size of 2.00mm and simulated in 

software. 

3.2 Simulation Results 

Figures 05 and 06 shows simulation result of Modified RMSA with straight edge cut. Three different graphs are 

combined showing variation in results for truncated length i.e. CUT equal to 3mm, 5mm and 7mm successively 

increasing by 2mm. From the figures 05 and 06 it can be observed that bandwidth of operation of antenna increases 

as CUT length increase. Due to physical limitations of radiating patch dimensions this truncation length can’t be 

further increased. 

The results observed from simulation of modified RMSA with straight edge cut are summarized in table 01. fL and fH 

indicate lower cut off and upper cut off frequency of the corresponding operating band in GHz. As cut length 

increases from No CUT to CUT length of 7.00mm, bandwidth is increase from 835.1 MHz to 5070.2 MHz. 

 

 

 

 

 

 

 

 

 

 

Figure 4. Structure of Modified RMSA with Straight Edge Cut(Type B) 

 

 

 

 

 

 

 

 

 

 

 

 

Figure 5. Return Loss vs. Frequency for modified RMSA with straight edge cut 



www.cribfb.com/journal/index.php/aijmsr           American International Journal of Multidisciplinary Scientific Research           Vol. 1, No. 1; 2018 

 

4 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

Figure 6.VSWR vs. Frequency for modified RMSA with straight edge cut 

4. Type C-Circular Edge Cut 

4.1 Type C- Circular Edge Cut Structure 

It is observed in previous section that, increase in discontinuity increases bandwidth of operation of an antenna. 

Truncation made with circular edges instead of straight edge will add more discontinuity. This can be achieved by 

intersecting circle of radius-‘RAD’ with radiating patch. All the dimensions of RMSA are kept constant as in 

previous design. Black portion in figure 7 shows radiating metal patch, while light gray portion is removed from the 

design. 

 

 

 

 

 

 

 

 

 

 

 

 

Figure 7. Structure of Modified RMSA with Circular Edge Cut(Type C) 

4.2 Simulation Results 

Figures 08 and 09 shows simulation result of Modified RMSA with Circular edge cut. Five different graphs are 

combined showing variation in results for truncation circle radius i.e. RAD equal to 13mm, 12mm, 11mm, 10mm 

and 9.2mm successively decreasing by 1mm. From the figures 08 and 09 it can be observed that bandwidth of 

operation of antenna increases as radius of intersecting circle decreases. In other words, bandwidth is inversely 

proportional to RAD. Benefit of using circular edge cut over straight edge cut can be observed. From RAD=11 two 

different bands of operation can be seen, one at lower frequency and other at higher frequency side of frequency axis 

which was not the case in straight edge cut. At Radius of 9.2mm total UWB band is covered by the structure. 
Table 02 summarizes results observed by variation in radius of truncating circle. Two distinct conclusions can be 
drawn from table 02. First with increase in truncating length i.e. decrease in RAD from 13 mm to 9.2mm, operating 
bandwidth increases from 835.1 MHz to 8947.4GHz covering entire UWB band of operation. Second conclusion 
drawn is related with the fact that two distinct operating bands are observed at lower and higher end of frequency 



www.cribfb.com/journal/index.php/aijmsr           American International Journal of Multidisciplinary Scientific Research           Vol. 1, No. 1; 2018 

 

5 

 

band at RAD=11mm and RAD=10mm. these two distinct bands come close to merge into each other and cover 
entire band starting from 3.0526 GHz to 12.00GHz. thus percent increase of 972% is observed in type C-antenna. 

 

 

 

 

 

 

 

 

 

 

 

 

 

 

Figure 8. Return Loss vs. Frequency for modified RMSA with circular edge cu 

 

 

 

 

 

 

 

 

Figure 09: VSWR vs. Frequency for modified RMSA with circular edge cut 

 

Figure 9. VSWR vs. Frequency for modified RMSA with circular edge cut 

 

Table 2. Comparison of Bandwidth of Modified RMSA with Circular edge cut (Type C) 

 

RAD(mm) fL (GHz) fH (GHz) Bandwidth(MHz) 

13.00 2.9632 3.7982 835.10 

12.00 3.0228 3.8877 864.90 

11.00 3.0526 4.0965 1043.90 

 7.7649 11.9702 4205.30 

10.00 3.0228 4.6632 1640.40 

 6.0649 12.0000 5935.10 

9.20 3.0526 12.0000 8947.40 

 

5. Conclusion 

Above simulated results and their comparison provides a brief idea of how narrow band simple RSMA can be 

transformed to Ultra Wide Band modified RSMA without changing its physical dimension. Circular edge 

truncation proves to be more efficient than straight edge truncation. Smoothening of corner of rectangle increases 

reflection and current at the boundary of patch. This lingering of current or wave must have improved bandwidth 

of antenna. Truncation of RSMA with circle of radius 9.2 mm leads to required UWB operation of antenna. 



www.cribfb.com/journal/index.php/aijmsr           American International Journal of Multidisciplinary Scientific Research           Vol. 1, No. 1; 2018 

 

6 

 

References 

H.N. Kritikos and D. L. Jaggard(1990).On fractal electrodynamics-Recent Advances in Electromagnetic Theory, 

Springer-Verlag, New York,183-224. 

Werner, D. H. and Ganguly S.,(2003).An overview of Fractal antenna engineering research, IEEE-Antenna and 

Propagation Magazine, 45(1),38-57. 

J. Liang, C. Chiau, X. Chen and J. Yu. (2004).Study of a circular disc monopole antennas for ultra wideband 

applications, International Symposium on Antennas and Propagation, 17-21 

J. Liang,et.al .(2005).CPW-fed circular disc monopole antenna for UWB application, IEEE International Workshop 

on Antenna and Technology:Small Antennas and Novel Meta materials, Marina Mandarin, Singapore, 

March 7–9, 505–508. 

Rick W. Kindt and William R. Pickles, Ultrawideband All-Metal Flared-Notch Array Radiator,(2010).IEEE Trans. 

On Antennas and Propagation, 58(11).50-56. 

Jiechen Ding,Zhili Lin,Zhinong Ying.(2007).A Compact Ultra Wideband Slot Antenna With Multiple Notch 

Frequency Bands, Microwave and optical Technology Letters,49(12). 

Min Ding et. al. (2007).Design of a CPW-fed Ultra Wideband Crown Circular Fractal Antenna. MOTL,173-176. 

M.Ramkumar Prabhu et al. (2017).Rectangular Patch Antenna to operate in flame retardant 4 using coaxial feeding 

technique in International Journal of Electronics Engineering Research. 9(3), 399-407 

  

 

 

Copyrights 

Copyright for this article is retained by the author(s), with first publication rights granted to the journal. 

This is an open-access article distributed under the terms and conditions of the Creative Commons Attribution 

license (http://creativecommons.org/licenses/by/4.0/) 

 


