id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajfst-1503	Tafa, Wabi; Olaniyan, Adesoji M	Design and Development of an Engine Driven Onion Grading Machine 	2023	14	.pdf	application/pdf	9235	473	64	The number of rotations per minute (Nc) found above is the critical speed at which falling ends and onion bulb remains in constant grading cylinder contact, held there by centrifugal force. W=mrc g (8) = 43.41 kg x 9.81m/s = 425.85 N Where: W = weight of the grading unit (N), mrc = mass of rotating grading cylinder (kg), and g = acceleration due to gravity (9.81m/s2).	cache/ajfst-1503.pdf	txt/ajfst-1503.txt
