id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
arees-4374	Ademila, Omowumi	Engineering Structural Strength Properties of Lateritic Soil-Cement Mix for Road Pavement Stability	2022	11	.pdf	application/pdf	5350	298	52	The UCS values of soil cement cured in 14 and 7 days (845.5 – 1011.6 and 761.7 – 872.1 kN/m2) are within the 750 – 1500 kN/m2 stipulated Nigerian General Specifications for highways [20] at 8% cement content. Keywords: Crushed rock, Curing period, Highway construction, Lateritic soil cement, Soil improvement, Structural properties.	cache/arees-4374.pdf	txt/arees-4374.txt
