id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
arees-6917	Elvira, Filatieva; Mikhail, Filatiev; Nikolay, Antoshchenko; Olha, Fursova; Inna, Maksyuk	Unsolved problems in the study of coal formation processes and the manifestation of hazardous properties of coal seams	2025	8	.pdf	application/pdf	5206	223	46	If some part is retained, the maximum gas content of anthracite coal seams can reach 45 m3 per ton of dry ash-free combustible mass (m3/tdacm), and that of coal seams - 35 m3/tdacm. Conclusions ....................................................................................................................................................................................... 12 References .............................................................................................................................................................................................. 12 mailto:elafilatyeva@gmail.com mailto:Mfilatev@gmail.com mailto:antm1949@gmail.com mailto:metmashdtu@gmail.com mailto:innagroys@gmail.com https://creativecommons.org/licenses/by/4.0/ https://creativecommons.org/licenses/by/4.0/ https://www.doi.org/10.20448/arees.v12i1.6917 https://orcid.org/0000-0002-1041-0535 https://orcid.org/0000-0001-5608-6737 https://orcid.org/0000-0001-8901-8263 https://orcid.org/0000-0002-9622-2622 https://orcid.org/0000-0002-0096-7372 Asian Review of Environmental and Earth Sciences, 2025, 12(1): 6-13 7 © 2025 by the authors; licensee Asian Online Journal Publishing Group Contribution of this paper to the literature The possibilities of forming dangerous properties of coal seams are considered not only at the stage of metamorphic transformations but also in relation to their occurrence, which is genetically connected with previous processes of accumulation of the initial material, subjected to successive transformations at different stages of coal formation.	cache/arees-6917.pdf	txt/arees-6917.txt
