id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
arees-696	OK, Edwin; BF, Alemaw; K, Laletsang; NT, Tafesse	Estimating Hydraulic Properties of Alluvial Sand Aquifer in Motloutse River course, Eastern Botswana	2017	8	.pdf	application/pdf	4987	257	53	[21] obtained a porosity of 35% for Motloutse River sand. In low loss medium (soils with low salinity and clay content) which is expected of river sand, the velocity (V) of the soil can be related to the dielectric constant by Eq. 1	cache/arees-696.pdf	txt/arees-696.txt
