id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
dss-63	Trakic, Ammar	Axial force coefficient of APFSDS projectile	2021-04-10	15	.pdf	application/pdf	5901	279	66	Axial force computation methods for projectile body The axial force of a projectile consists of the pressure axial force of the nose, base (including possible tail boom), protruding (driving band, grooves and steps), and of the viscous axial force as a sum of the following form [6]: 𝐶 = 𝐶 + 𝐶 + 𝐶 + 𝐶 (2) where 𝐶 is axial force coefficient of the nose, 𝐶 is axial force coefficient of the base, 𝐶 is axial force coefficient of the protruding and 𝐶 is viscous axial force coefficient. The total axial force coefficient of APFSDS projectile (without sabot) is [6]: 𝐶 = 𝐶 + 𝐶 (1) where 𝐶 is axial force coefficient of projectile body and 𝐶 is axial force coefficient of fins.	cache/dss-63.pdf	txt/dss-63.txt
