id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
eaes-25157	Sani, Abdoulwahid; Baraou Idi, Souley	Geophysical Mapping by Electromagnetic Induction of Gold Occurrences in Birimian Formations of Liptako: Case of Sorbon Haoussa Sector (Souhwest Niger)	2023	16	.pdf	application/pdf	3645	160	58	The interpretation of obtained results shown two types of resistive anomalies, corresponding to the conductive units: deep anomalies obtained with low frequencies and subsurface anomalies detected with high frequencies. The PROMIS-10 system used in this work is a new multi-frequency electromagnetic induction technology that can send up to 10 frequencies up to 14 080 Hz, 28160 Hz and 56320 Hz for high frequencies.	cache/eaes-25157.pdf	txt/eaes-25157.txt
