id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
fuen-122	Shaghaghi, Aidin ; Eskandarpanah, Reza ; Gitifar, Siavash; Zahedi, Rahim; Pourrahmani, Hossein; Keshavarzzade, Mansour; Ahmadi, Abolfazl	Energy consumption reduction in a building by free cooling using phase change material (PCM)	2023	6	.pdf	application/pdf	4132	195	54	The process of discharging cooling energy According to the profile of ambient air temperature during the day for Zanjan, the cooling energy discharge process has been studied in the following four different conditions. Then, a free cooling system using commercial paraffin RT25 was numerically analyzed as phase change material (PCM) while investigating the effects of the flow rate of the storage tank and inlet air temperature overcharging and discharging procedures.	cache/fuen-122.pdf	txt/fuen-122.txt
