id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
cord-264152-0jr5nlli	Bhattacharya, Raj Kumar	Sub-basin prioritization for assessment of soil erosion susceptibility in Kangsabati, a plateau basin: A comparison between MCDM and SWAT models	2020-05-16		.txt	text/plain	5756	159	30	1000 iterations were used for the determination of following parameters, where 500 iterations for flow parameters (10×50 per iteration), and 500 iterations for sediment parameters (10×50 per iteration) were required with the help of SWAT-CUP software. Therefore, VIKOR reflects the significant role of morphometric parameters on ES, whereas SWAT reflects the significant role of LULC, slope, and soil on ES.	cache/cord-264152-0jr5nlli.txt	txt/cord-264152-0jr5nlli.txt
