id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajee-3266	Saifullah, Mohammad; Hasan, Mehedi; Debnath, Tarun; Rob, M A; Tusar, Azizul Hakim; Rabbani, Md. Liton	Investigation the Use of Waste Glass and Waste Paper as an Alternative Construction Binding Material: An Approach Towards Sustainable Environment	2024	15	.pdf	application/pdf	7561	395	48	At just 7 days of curing, concrete blocks incorporating 10% and 20% glass waste replacements displayed higher strength than their conventional counterparts, showcasing an early strength advantage. These findings suggest that at 7 days of curing, lower percentages of waste glass replacement can enhance the strength of the concrete block, while at 14 days of curing, the strength remains close to the standard value for 10% and 20% replacement but decreases significantly at 30% replacement.	cache/ajee-3266.pdf	txt/ajee-3266.txt
