id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
ajfst-1508	Hailu, Getachew	Adaptation and Performance Evaluation Closed Drum Type Carbonizer for Waste Biomass	2023	6	.pdf	application/pdf	2898	137	47	At ten-minute intervals, temperatures were measured at each location, and the data were recorded. RESULTS AND DISCUSSION Carbonizer Selection Based on an evaluation of the various carbonizer designs already in existence, the best design of carbonizer for the carbonization of refuse sawdust and coffee husk was chosen. Various agricultural waste products (such as sawdust, coffee husks, peanut shells, and millet stalks) have been heated up in a device called a carbonizer.	cache/ajfst-1508.pdf	txt/ajfst-1508.txt
