id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
dss-212	A. Zaldiansyah; Widianto, N. ; Yogaswara, Y. H. ; Ruyat, Y. 	Analysis of Importance Priority to be Studied on Igniter System of 450 caliber X Rocket 	2022-12-30	4	.pdf	application/pdf	1933	74	51	List Of Requirements (LOR) Instruments User Requirements Urgency Power supply Electric current requirement of 1 Ampere and voltage requirement of 20 Volt 4 Switch connector An emergency system is needed in the electrical panel box to be able to immediately cut off the current when something unexpected happens 5 Cable Proper cable are needed for 1 Ampere and 20 Volts, and have low resistance so that the time delay in igniter operation can be cut 4 Grounding The grounding system required when operating the igniter is integrated with the firing system, and is expected to have a minimal resistance value, so that the static electricity contained in the wiring can be wasted towards ground 3 Casing The main casing needs are the Melting Point of 600°C, the distribution of combustion is even, and the casing melts instantly 5 Squib It takes a squib that has a long shelf life, and is not easily oxidized at room temperature 3 Squib Explosives Requires high calorific value, low flameability 4 Propellant Material It requires a high calorific value, with the same flameability as that produced by an igniter flame 4 Igniter explosives Requires high calorific value, low flameability 4 Description for Table 1: • Score 1: Not important.	cache/dss-212.pdf	txt/dss-212.txt
