id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
fuen-222	Das, Simul ; Rahman, Md. Arafat ; Islam, Md. Saiful ; Bhowmik, Konok Chandra 	Experimental investigation of cycling characteristics of anatase TiO2 nanotubes as negative electrode of lithium-ion batteries	2024	7	.pdf	application/pdf	3569	222	57	Our analysis covered a 2θ range from 10 o to 90 o with a step size of 0.05o, utilizing Cu Kα radiation (Empyrean, Panalytical-Netherlands) with a wavelength of ƛ = 1.5406Å. The morphological and compositional characterization of anatase TiO2 nanotubes was carried out using scanning electron microscopy and energy dispersive X-ray spectroscopy (SEM-EDX). 3. Results & discussion 3.1 XRD analysis As illustrated in Figure 2, the X-ray diffraction (XRD) technique is used to analyze the phase purity and crystallinity of Ti and anatase TiO2 nanotubes.	cache/fuen-222.pdf	txt/fuen-222.txt
