id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
cord-007363-h8xa83nw	Yan, Yihuan	Numerical investigation of indoor particulate contaminant transport using the Eulerian-Eulerian and Eulerian-Lagrangian two-phase flow models	2019-05-09		.txt	text/plain	5363	189	47	The models were compared against each other in the aspects of air velocity, particle concentration, and particle-wall interactions. It was found that the two models have similar accuracy in predicting the airflow field while each of them has its own advantage and drawback in modelling particle concentration and particle-wall interactions.	cache/cord-007363-h8xa83nw.txt	txt/cord-007363-h8xa83nw.txt
