id	author	title	date	pages	extension	mime	words	sentence	flesch	summary	cache	txt
21531	Fairham, William	Woodwork Joints: How They Are Set Out, How Made and Where Used.			.txt	text/plain	37265	2423	81	A joint of this type may be applied in nearly all cases where a halved or a mortise and tenon joint could be used. This is also called an Open slot mortise and tenon joint, a good strong, serviceable joint which can be used instead of the closed mortise and tenon type, its advantage being that less labour is required in the making.	cache/21531.txt	txt/21531.txt
